Topic : ☐ 대기환경 ☑ 수질환경  ☐ 실내환경 ☐ 산업보건 ☐ 환경독성 ☐ 환경위생 ☐ 건강영향 ☐ 노출 및 위해도평가

통계분석법을 이용한 서울시 물재생센터의 수질평가

Statistical Evaluation on Water Quality of Municipal Wastewater Treatment Plants in Seoul, Korea

이진1, 이준연1, 최예덕1, 홍주희1, 이순희1, 안정희1, 이효진1, 한규문1, 이목영1, 정권1

1서울시보건환경연구원

(발표자 : wisegenie@seoul.go.kr)

[서론] 도시에서 발생하는 우수와 오수를 배제 또는 처리하기 위하여 설치된 물재생센터는 도시의 물순환에 중요한 역할을 하고 있다. 현재 운전되고 있는 물재생센터는 설계시 대상처리공정의 운영면에서 유입수질 대비 방류수질 비율, 방류수 수질 기준 초과 여부 등으로 처리 성능을 평가하고 있다. 변동적인 특성을 지닌 물재생센터의 유입수와 방류수의 수질을 통계적인 기법을 도입하여 계절적, 공간적 처리효율을 분석하고자 한다.

[연구방법] 서울시는 한강과 주요하천 4개소(홍제천, 중랑천, 탄천, 안양천)를 중심으로 강남지역과 강북지역으로 분할하고 이를 동·서쪽으로 나누어 총4개의 처리구역으로 구분하여 4개의 물재생센터에서 하수를 처리하고 있다. 4개의 물재생센터의 유입수와 방류수 수질 모니터링 자료 (2014-2016년)는 서울시 물재생시설과로부터 구하였으며, 통계분석은 SAS v8 package (SAS Inst., Cary, NC)을 이용하여 분석하였다.

[연구결과 및 고찰] 물재생센터의 유입수의 표준편차는 0.6-31.7 mg/L로 평균농도 대비 약 16.2-22.4%의 범위를 보였으며 BOD와 SS가 상대적으로 큰 편차를 보였다. 방류수의 경우 전항목에 걸쳐 표준편차는 0.6-3.3 mg/L로 평균농도 대비 24.8-100%의 범위를 보였으며 SS의 변동이 큰 것으로 나타났다. BOD, COD, SS, TN 그리고 TP의 처리효육은 계절적 그리고 공간적인 변동이 상당하였다 (p<0.001).

Fig.1 Removal efficiencies of water quality parameters in each season	Fig.2 Removal efficiencies of water quality parameters in each wastewater treatment plant

[참고문헌]

Choi LC, Ahn SJ, Chung HM, Kwon OS, Kim WK, Yeom IT, Son DH. A study on the evaluation for operations of public sewage treatment plans using statistics technique. Journal of Korean Society on Water Environment. 2014; 30(5): 524-531.