HOIST 50UNIT  INSPECTION

REV:004 (2015.07.30)

순번	검 사 항 목	참 조 및 UNIT	상태 및 조치	작업자	검사자
1	ELECTRIC HOIST GOODRICH FRANCE - Greasing of the winder screw. - Check the cable. - Check the extract and winding cable. - Check the hook. - Check the functioning idle(s) and ends of travel.	CMM 25.64.99 SECTION 500 6M // 50HC Margin :0/0
2	D’LOK HOOK - Carefully inspect the entire D’LOK hook, in particular the lock latch gate, for aspect, cleanliness, absence of damage(distortion, cracks), unusual wears and corrosion. Check the proper operation of the D’LOK hook opening. Check that the drainage hole is not blocked. Check the free rotation of the hook part. If necessary, clean with mild soap and water, thoroughly rince and allow to completely dry. Spray a water repellant product, ARDROX3965, (or equivalent) on the inner mechanism of the hook latch gate. Remove excess of product.	6M // 50HC GOODRICH SB 76378-25-08

주) HC = Hoist Cycle

- 1 – End